(export 
  (version "E") 
  (design 
    (source "Z:\\FritzNAS_USB500\\__Share and Xchange\\___KiCad-Projekte\\ZisternenFüllstand v1.0\\ZisternenFüllstand v1.0.kicad_sch") 
    (date "2024-04-08T12:20:40+0200") 
    (tool "Eeschema 8.0.1") 
    (sheet 
      (number "1") 
      (name "/") 
      (tstamps "/") 
      (title_block 
        (title) 
        (company) 
        (rev "1.0") 
        (date "2024-04-03") 
        (source "ZisternenFüllstand v1.0.kicad_sch") 
        (comment 
          (number "1") 
          (value "")) 
        (comment 
          (number "2") 
          (value "")) 
        (comment 
          (number "3") 
          (value "")) 
        (comment 
          (number "4") 
          (value "")) 
        (comment 
          (number "5") 
          (value "")) 
        (comment 
          (number "6") 
          (value "")) 
        (comment 
          (number "7") 
          (value "")) 
        (comment 
          (number "8") 
          (value "")) 
        (comment 
          (number "9") 
          (value ""))))) 
  (components 
    (comp 
      (ref "A1") 
      (value "PinSocket_1x15_2.54") 
      (footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description"))) 
      (libsource 
        (lib "_Lp-Bauteile") 
        (part "Conn_01x15_1") 
        (description "")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "afda77b1-250e-4766-928f-b900164047f3")) 
    (comp 
      (ref "A2") 
      (value "PinSocket_1x15_2.54") 
      (footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description"))) 
      (libsource 
        (lib "Connector_Generic") 
        (part "Conn_01x15") 
        (description "Generic connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "00000000-0000-0000-0000-000056d71a21")) 
    (comp 
      (ref "C1") 
      (value "100nF") 
      (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm") 
      (description "Unpolarized capacitor, small symbol") 
      (fields 
        (field 
          (name "Footprint") "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Unpolarized capacitor, small symbol")) 
      (libsource 
        (lib "Device") 
        (part "C_Small") 
        (description "Unpolarized capacitor, small symbol")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "capacitor cap")) 
      (property 
        (name "ki_fp_filters") 
        (value "C_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "44f4382a-ddfa-4969-be0d-9212fea66881")) 
    (comp 
      (ref "C2") 
      (value "10uF/36V") 
      (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm") 
      (description "Polarized capacitor") 
      (fields 
        (field 
          (name "Footprint") "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Polarized capacitor")) 
      (libsource 
        (lib "Device") 
        (part "C_Polarized") 
        (description "Polarized capacitor")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "cap capacitor")) 
      (property 
        (name "ki_fp_filters") 
        (value "CP_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "67fef9ae-0e7d-455e-aebb-52c14c1260e2")) 
    (comp 
      (ref "C3") 
      (value "10uF/16V") 
      (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm") 
      (description "Polarized capacitor") 
      (fields 
        (field 
          (name "Footprint") "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Polarized capacitor")) 
      (libsource 
        (lib "Device") 
        (part "C_Polarized") 
        (description "Polarized capacitor")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "cap capacitor")) 
      (property 
        (name "ki_fp_filters") 
        (value "CP_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "d48c37ce-9a24-4fd7-ad3e-edd456d44d72")) 
    (comp 
      (ref "C4") 
      (value "100nF") 
      (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm") 
      (description "Unpolarized capacitor, small symbol") 
      (fields 
        (field 
          (name "Footprint") "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Unpolarized capacitor, small symbol")) 
      (libsource 
        (lib "Device") 
        (part "C_Small") 
        (description "Unpolarized capacitor, small symbol")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "capacitor cap")) 
      (property 
        (name "ki_fp_filters") 
        (value "C_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "fc8c0597-aa74-4ed0-9620-e76a8e1d7ba6")) 
    (comp 
      (ref "D1") 
      (value "1N4007") 
      (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal") 
      (datasheet "http://www.vishay.com/docs/88503/1n4001.pdf") 
      (description "1000V 1A General Purpose Rectifier Diode, DO-41") 
      (fields 
        (field 
          (name "Sim.Device") "D") 
        (field 
          (name "Sim.Pins") "1=K 2=A") 
        (field 
          (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal") 
        (field 
          (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf") 
        (field 
          (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41")) 
      (libsource 
        (lib "Diode") 
        (part "1N4007") 
        (description "1000V 1A General Purpose Rectifier Diode, DO-41")) 
      (property 
        (name "Sim.Device") 
        (value "D")) 
      (property 
        (name "Sim.Pins") 
        (value "1=K 2=A")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "diode")) 
      (property 
        (name "ki_fp_filters") 
        (value "D*DO?41*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "91093476-7b56-465b-a561-cea18cd249d4")) 
    (comp 
      (ref "J1") 
      (value "Screw_Terminal_01x02") 
      (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical") 
      (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")) 
      (libsource 
        (lib "Connector") 
        (part "Screw_Terminal_01x02") 
        (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "screw terminal")) 
      (property 
        (name "ki_fp_filters") 
        (value "TerminalBlock*:*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "5081d023-d866-48c2-a27d-5765bd8dfdf0")) 
    (comp 
      (ref "J2") 
      (value "Jack-DC") 
      (footprint "Connector_BarrelJack:BarrelJack_Horizontal") 
      (description "DC Barrel Jack") 
      (fields 
        (field 
          (name "Footprint") "Connector_BarrelJack:BarrelJack_Horizontal") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "DC Barrel Jack")) 
      (libsource 
        (lib "Connector") 
        (part "Jack-DC") 
        (description "DC Barrel Jack")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "DC power barrel jack connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "BarrelJack*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "dd8e6572-eb6e-4e20-9e43-373e91c0f40b")) 
    (comp 
      (ref "J3") 
      (value "Conn_01x02_Pin") 
      (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical") 
      (description "Generic connector, single row, 01x02, script generated") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Generic connector, single row, 01x02, script generated")) 
      (libsource 
        (lib "Connector") 
        (part "Conn_01x02_Pin") 
        (description "Generic connector, single row, 01x02, script generated")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "573d1a82-3197-4522-a365-e7060c08994e")) 
    (comp 
      (ref "L1") 
      (value "L7805") 
      (footprint "Package_TO_SOT_THT:TO-220-3_Vertical") 
      (datasheet "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf") 
      (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252") 
      (fields 
        (field 
          (name "Footprint") "Package_TO_SOT_THT:TO-220-3_Vertical") 
        (field 
          (name "Datasheet") "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf") 
        (field 
          (name "Description") "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")) 
      (libsource 
        (lib "Regulator_Linear") 
        (part "L7805") 
        (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "Voltage Regulator 1.5A Positive")) 
      (property 
        (name "ki_fp_filters") 
        (value "TO?252* TO?263* TO?220*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "ece05432-4c8f-427a-aa5c-ada60ef1b409")) 
    (comp 
      (ref "R1") 
      (value "4k7") 
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal") 
      (description "Resistor") 
      (fields 
        (field 
          (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Resistor")) 
      (libsource 
        (lib "Device") 
        (part "R") 
        (description "Resistor")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "R res resistor")) 
      (property 
        (name "ki_fp_filters") 
        (value "R_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "8236a14e-fac8-4b0b-841a-3130a9472569")) 
    (comp 
      (ref "U1") 
      (value "18B20") 
      (footprint "Package_TO_SOT_THT:TO-92_Inline") 
      (datasheet "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf") 
      (description "Programmable Resolution 1-Wire Digital Thermometer TO-92") 
      (fields 
        (field 
          (name "Footprint") "Package_TO_SOT_THT:TO-92_Inline") 
        (field 
          (name "Datasheet") "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf") 
        (field 
          (name "Description") "Programmable Resolution 1-Wire Digital Thermometer TO-92")) 
      (libsource 
        (lib "Sensor_Temperature") 
        (part "DS18B20") 
        (description "Programmable Resolution 1-Wire Digital Thermometer TO-92")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "OneWire 1Wire Dallas Maxim")) 
      (property 
        (name "ki_fp_filters") 
        (value "TO*92*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "938caf0c-d9e5-4afc-9c03-5e7b41a2e97f")) 
    (comp 
      (ref "X1") 
      (value "DS18B20") 
      (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal") 
      (description "Generic connector, single row, 01x03, script generated") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Generic connector, single row, 01x03, script generated")) 
      (libsource 
        (lib "Connector") 
        (part "Conn_01x03_Pin") 
        (description "Generic connector, single row, 01x03, script generated")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "dbcd608d-3ff2-49c2-bd35-565c9bee3116")) 
    (comp 
      (ref "X1C1") 
      (value "Conn_01x04_Socket") 
      (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical") 
      (description "Generic connector, single row, 01x04, script generated") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Generic connector, single row, 01x04, script generated")) 
      (libsource 
        (lib "Connector") 
        (part "Conn_01x04_Socket") 
        (description "Generic connector, single row, 01x04, script generated")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "ffd66371-90be-400b-bc38-e9e594c2f2e1")) 
    (comp 
      (ref "X1L1") 
      (value "Conn_01x04_Socket") 
      (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical") 
      (description "Generic connector, single row, 01x04, script generated") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Generic connector, single row, 01x04, script generated")) 
      (libsource 
        (lib "Connector") 
        (part "Conn_01x04_Socket") 
        (description "Generic connector, single row, 01x04, script generated")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "842732d0-2946-47ff-8166-44a538666d2f")) 
    (comp 
      (ref "X2") 
      (value "Conn_01x04_Socket") 
      (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal") 
      (description "Generic connector, single row, 01x04, script generated") 
      (fields 
        (field 
          (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal") 
        (field 
          (name "Datasheet")) 
        (field 
          (name "Description") "Generic connector, single row, 01x04, script generated")) 
      (libsource 
        (lib "Connector") 
        (part "Conn_01x04_Socket") 
        (description "Generic connector, single row, 01x04, script generated")) 
      (property 
        (name "Sheetname") 
        (value "Stammblatt")) 
      (property 
        (name "Sheetfile") 
        (value "ZisternenFüllstand v1.0.kicad_sch")) 
      (property 
        (name "ki_keywords") 
        (value "connector")) 
      (property 
        (name "ki_fp_filters") 
        (value "Connector*:*_1x??_*")) 
      (sheetpath 
        (names "/") 
        (tstamps "/")) 
      (tstamps "f8c149e8-89f9-4f0b-8312-a11ce1fe99ac"))) 
  (libparts 
    (libpart 
      (lib "Connector") 
      (part "Conn_01x02_Pin") 
      (description "Generic connector, single row, 01x02, script generated") 
      (docs "~") 
      (footprints 
        (fp "Connector*:*_1x??_*")) 
      (fields 
        (field 
          (name "Reference") "J") 
        (field 
          (name "Value") "Conn_01x02_Pin") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Generic connector, single row, 01x02, script generated")) 
      (pins 
        (pin 
          (num "1") 
          (name "Pin_1") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "Pin_2") 
          (type "passive")))) 
    (libpart 
      (lib "Connector") 
      (part "Conn_01x03_Pin") 
      (description "Generic connector, single row, 01x03, script generated") 
      (docs "~") 
      (footprints 
        (fp "Connector*:*_1x??_*")) 
      (fields 
        (field 
          (name "Reference") "J") 
        (field 
          (name "Value") "Conn_01x03_Pin") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Generic connector, single row, 01x03, script generated")) 
      (pins 
        (pin 
          (num "1") 
          (name "Pin_1") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "Pin_2") 
          (type "passive")) 
        (pin 
          (num "3") 
          (name "Pin_3") 
          (type "passive")))) 
    (libpart 
      (lib "Connector") 
      (part "Conn_01x04_Socket") 
      (description "Generic connector, single row, 01x04, script generated") 
      (docs "~") 
      (footprints 
        (fp "Connector*:*_1x??_*")) 
      (fields 
        (field 
          (name "Reference") "J") 
        (field 
          (name "Value") "Conn_01x04_Socket") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Generic connector, single row, 01x04, script generated")) 
      (pins 
        (pin 
          (num "1") 
          (name "Pin_1") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "Pin_2") 
          (type "passive")) 
        (pin 
          (num "3") 
          (name "Pin_3") 
          (type "passive")) 
        (pin 
          (num "4") 
          (name "Pin_4") 
          (type "passive")))) 
    (libpart 
      (lib "Connector") 
      (part "Jack-DC") 
      (description "DC Barrel Jack") 
      (docs "~") 
      (footprints 
        (fp "BarrelJack*")) 
      (fields 
        (field 
          (name "Reference") "J") 
        (field 
          (name "Value") "Jack-DC") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "DC Barrel Jack")) 
      (pins 
        (pin 
          (num "1") 
          (name "") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "") 
          (type "passive")))) 
    (libpart 
      (lib "Connector") 
      (part "Screw_Terminal_01x02") 
      (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)") 
      (docs "~") 
      (footprints 
        (fp "TerminalBlock*:*")) 
      (fields 
        (field 
          (name "Reference") "J") 
        (field 
          (name "Value") "Screw_Terminal_01x02") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")) 
      (pins 
        (pin 
          (num "1") 
          (name "Pin_1") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "Pin_2") 
          (type "passive")))) 
    (libpart 
      (lib "Connector_Generic") 
      (part "Conn_01x15") 
      (description "Generic connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)") 
      (docs "~") 
      (footprints 
        (fp "Connector*:*_1x??_*")) 
      (fields 
        (field 
          (name "Reference") "J") 
        (field 
          (name "Value") "Conn_01x15") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Generic connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)")) 
      (pins 
        (pin 
          (num "1") 
          (name "Pin_1") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "Pin_2") 
          (type "passive")) 
        (pin 
          (num "3") 
          (name "Pin_3") 
          (type "passive")) 
        (pin 
          (num "4") 
          (name "Pin_4") 
          (type "passive")) 
        (pin 
          (num "5") 
          (name "Pin_5") 
          (type "passive")) 
        (pin 
          (num "6") 
          (name "Pin_6") 
          (type "passive")) 
        (pin 
          (num "7") 
          (name "Pin_7") 
          (type "passive")) 
        (pin 
          (num "8") 
          (name "Pin_8") 
          (type "passive")) 
        (pin 
          (num "9") 
          (name "Pin_9") 
          (type "passive")) 
        (pin 
          (num "10") 
          (name "Pin_10") 
          (type "passive")) 
        (pin 
          (num "11") 
          (name "Pin_11") 
          (type "passive")) 
        (pin 
          (num "12") 
          (name "Pin_12") 
          (type "passive")) 
        (pin 
          (num "13") 
          (name "Pin_13") 
          (type "passive")) 
        (pin 
          (num "14") 
          (name "Pin_14") 
          (type "passive")) 
        (pin 
          (num "15") 
          (name "Pin_15") 
          (type "passive")))) 
    (libpart 
      (lib "Device") 
      (part "C_Polarized") 
      (description "Polarized capacitor") 
      (docs "~") 
      (footprints 
        (fp "CP_*")) 
      (fields 
        (field 
          (name "Reference") "C") 
        (field 
          (name "Value") "C_Polarized") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Polarized capacitor")) 
      (pins 
        (pin 
          (num "1") 
          (name "") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "") 
          (type "passive")))) 
    (libpart 
      (lib "Device") 
      (part "C_Small") 
      (description "Unpolarized capacitor, small symbol") 
      (docs "~") 
      (footprints 
        (fp "C_*")) 
      (fields 
        (field 
          (name "Reference") "C") 
        (field 
          (name "Value") "C_Small") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Unpolarized capacitor, small symbol")) 
      (pins 
        (pin 
          (num "1") 
          (name "") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "") 
          (type "passive")))) 
    (libpart 
      (lib "Device") 
      (part "R") 
      (description "Resistor") 
      (docs "~") 
      (footprints 
        (fp "R_*")) 
      (fields 
        (field 
          (name "Reference") "R") 
        (field 
          (name "Value") "R") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description") "Resistor")) 
      (pins 
        (pin 
          (num "1") 
          (name "") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "") 
          (type "passive")))) 
    (libpart 
      (lib "Diode") 
      (part "1N4007") 
      (description "1000V 1A General Purpose Rectifier Diode, DO-41") 
      (docs "http://www.vishay.com/docs/88503/1n4001.pdf") 
      (footprints 
        (fp "D*DO?41*")) 
      (fields 
        (field 
          (name "Reference") "D") 
        (field 
          (name "Value") "1N4007") 
        (field 
          (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal") 
        (field 
          (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf") 
        (field 
          (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41") 
        (field 
          (name "Sim.Device") "D") 
        (field 
          (name "Sim.Pins") "1=K 2=A")) 
      (pins 
        (pin 
          (num "1") 
          (name "K") 
          (type "passive")) 
        (pin 
          (num "2") 
          (name "A") 
          (type "passive")))) 
    (libpart 
      (lib "Regulator_Linear") 
      (part "L7805") 
      (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252") 
      (docs "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf") 
      (footprints 
        (fp "TO?252*") 
        (fp "TO?263*") 
        (fp "TO?220*")) 
      (fields 
        (field 
          (name "Reference") "U") 
        (field 
          (name "Value") "L7805") 
        (field 
          (name "Footprint")) 
        (field 
          (name "Datasheet") "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf") 
        (field 
          (name "Description") "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")) 
      (pins 
        (pin 
          (num "1") 
          (name "IN") 
          (type "power_in")) 
        (pin 
          (num "2") 
          (name "GND") 
          (type "power_in")) 
        (pin 
          (num "3") 
          (name "OUT") 
          (type "power_out")))) 
    (libpart 
      (lib "Sensor_Temperature") 
      (part "DS18B20") 
      (description "Programmable Resolution 1-Wire Digital Thermometer TO-92") 
      (docs "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf") 
      (footprints 
        (fp "TO*92*")) 
      (fields 
        (field 
          (name "Reference") "U") 
        (field 
          (name "Value") "DS18B20") 
        (field 
          (name "Footprint") "Package_TO_SOT_THT:TO-92_Inline") 
        (field 
          (name "Datasheet") "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf") 
        (field 
          (name "Description") "Programmable Resolution 1-Wire Digital Thermometer TO-92")) 
      (pins 
        (pin 
          (num "1") 
          (name "GND") 
          (type "power_in")) 
        (pin 
          (num "2") 
          (name "DQ") 
          (type "bidirectional")) 
        (pin 
          (num "3") 
          (name "V_{DD}") 
          (type "power_in")))) 
    (libpart 
      (lib "_Lp-Bauteile") 
      (part "Conn_01x15_1") 
      (docs "~") 
      (footprints 
        (fp "Connector*:*_1x??_*")) 
      (fields 
        (field 
          (name "Reference") "J?") 
        (field 
          (name "Value") "Analog") 
        (field 
          (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical") 
        (field 
          (name "Datasheet") "~") 
        (field 
          (name "Description"))) 
      (pins 
        (pin 
          (num "16") 
          (name "Pin_16") 
          (type "passive")) 
        (pin 
          (num "17") 
          (name "Pin_17") 
          (type "passive")) 
        (pin 
          (num "18") 
          (name "Pin_18") 
          (type "passive")) 
        (pin 
          (num "19") 
          (name "Pin_19") 
          (type "passive")) 
        (pin 
          (num "20") 
          (name "Pin_20") 
          (type "passive")) 
        (pin 
          (num "21") 
          (name "Pin_21") 
          (type "passive")) 
        (pin 
          (num "22") 
          (name "Pin_22") 
          (type "passive")) 
        (pin 
          (num "23") 
          (name "Pin_23") 
          (type "passive")) 
        (pin 
          (num "24") 
          (name "Pin_24") 
          (type "passive")) 
        (pin 
          (num "25") 
          (name "Pin_25") 
          (type "passive")) 
        (pin 
          (num "26") 
          (name "Pin_26") 
          (type "passive")) 
        (pin 
          (num "27") 
          (name "Pin_27") 
          (type "passive")) 
        (pin 
          (num "28") 
          (name "Pin_28") 
          (type "passive")) 
        (pin 
          (num "29") 
          (name "Pin_29") 
          (type "passive")) 
        (pin 
          (num "30") 
          (name "Pin_30") 
          (type "passive"))))) 
  (libraries 
    (library 
      (logical "Connector") 
      (uri "C:\\Program Files\\KiCad\\8.0\\share\\kicad\\symbols\\/Connector.kicad_sym")) 
    (library 
      (logical "Connector_Generic") 
      (uri "C:\\Program Files\\KiCad\\8.0\\share\\kicad\\symbols\\/Connector_Generic.kicad_sym")) 
    (library 
      (logical "Device") 
      (uri "C:\\Program Files\\KiCad\\8.0\\share\\kicad\\symbols\\/Device.kicad_sym")) 
    (library 
      (logical "Diode") 
      (uri "C:\\Program Files\\KiCad\\8.0\\share\\kicad\\symbols\\/Diode.kicad_sym")) 
    (library 
      (logical "Regulator_Linear") 
      (uri "C:\\Program Files\\KiCad\\8.0\\share\\kicad\\symbols\\/Regulator_Linear.kicad_sym")) 
    (library 
      (logical "Sensor_Temperature") 
      (uri "C:\\Program Files\\KiCad\\8.0\\share\\kicad\\symbols\\/Sensor_Temperature.kicad_sym"))) 
  (nets 
    (net 
      (code "1") 
      (name "+5V") 
      (node 
        (ref "A1") 
        (pin "27") 
        (pinfunction "Pin_27") 
        (pintype "passive")) 
      (node 
        (ref "C3") 
        (pin "1") 
        (pintype "passive")) 
      (node 
        (ref "C4") 
        (pin "1") 
        (pintype "passive")) 
      (node 
        (ref "L1") 
        (pin "3") 
        (pinfunction "OUT") 
        (pintype "power_out")) 
      (node 
        (ref "R1") 
        (pin "1") 
        (pintype "passive")) 
      (node 
        (ref "X1") 
        (pin "3") 
        (pinfunction "Pin_3") 
        (pintype "passive")) 
      (node 
        (ref "X1C1") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive")) 
      (node 
        (ref "X1L1") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive")) 
      (node 
        (ref "X2") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive"))) 
    (net 
      (code "2") 
      (name "/*D3") 
      (node 
        (ref "A2") 
        (pin "6") 
        (pinfunction "Pin_6") 
        (pintype "passive")) 
      (node 
        (ref "X2") 
        (pin "3") 
        (pinfunction "Pin_3") 
        (pintype "passive"))) 
    (net 
      (code "3") 
      (name "/*D10{slash}SS") 
      (node 
        (ref "A2") 
        (pin "13") 
        (pinfunction "Pin_13") 
        (pintype "passive")) 
      (node 
        (ref "R1") 
        (pin "2") 
        (pintype "passive")) 
      (node 
        (ref "U1") 
        (pin "2") 
        (pinfunction "DQ") 
        (pintype "bidirectional")) 
      (node 
        (ref "X1") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive"))) 
    (net 
      (code "4") 
      (name "/A4{slash}SDA") 
      (node 
        (ref "A1") 
        (pin "23") 
        (pinfunction "Pin_23") 
        (pintype "passive")) 
      (node 
        (ref "X1C1") 
        (pin "4") 
        (pinfunction "Pin_4") 
        (pintype "passive")) 
      (node 
        (ref "X1L1") 
        (pin "4") 
        (pinfunction "Pin_4") 
        (pintype "passive"))) 
    (net 
      (code "5") 
      (name "/A5{slash}SCL") 
      (node 
        (ref "A1") 
        (pin "24") 
        (pinfunction "Pin_24") 
        (pintype "passive")) 
      (node 
        (ref "X1C1") 
        (pin "3") 
        (pinfunction "Pin_3") 
        (pintype "passive")) 
      (node 
        (ref "X1L1") 
        (pin "3") 
        (pinfunction "Pin_3") 
        (pintype "passive"))) 
    (net 
      (code "6") 
      (name "/D2") 
      (node 
        (ref "A2") 
        (pin "5") 
        (pinfunction "Pin_5") 
        (pintype "passive")) 
      (node 
        (ref "X2") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive"))) 
    (net 
      (code "8") 
      (name "GND") 
      (node 
        (ref "A1") 
        (pin "29") 
        (pinfunction "Pin_29") 
        (pintype "passive")) 
      (node 
        (ref "A2") 
        (pin "4") 
        (pinfunction "Pin_4") 
        (pintype "passive")) 
      (node 
        (ref "C1") 
        (pin "2") 
        (pintype "passive")) 
      (node 
        (ref "C2") 
        (pin "2") 
        (pintype "passive")) 
      (node 
        (ref "C3") 
        (pin "2") 
        (pintype "passive")) 
      (node 
        (ref "C4") 
        (pin "2") 
        (pintype "passive")) 
      (node 
        (ref "J1") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive")) 
      (node 
        (ref "J2") 
        (pin "2") 
        (pintype "passive")) 
      (node 
        (ref "L1") 
        (pin "2") 
        (pinfunction "GND") 
        (pintype "power_in")) 
      (node 
        (ref "U1") 
        (pin "1") 
        (pinfunction "GND") 
        (pintype "power_in")) 
      (node 
        (ref "U1") 
        (pin "3") 
        (pinfunction "V_{DD}") 
        (pintype "power_in")) 
      (node 
        (ref "X1") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive")) 
      (node 
        (ref "X1C1") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive")) 
      (node 
        (ref "X1L1") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive")) 
      (node 
        (ref "X2") 
        (pin "4") 
        (pinfunction "Pin_4") 
        (pintype "passive"))) 
    (net 
      (code "9") 
      (name "Net-(D1-A)") 
      (node 
        (ref "D1") 
        (pin "2") 
        (pinfunction "A") 
        (pintype "passive")) 
      (node 
        (ref "J3") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive"))) 
    (net 
      (code "10") 
      (name "Net-(D1-K)") 
      (node 
        (ref "C1") 
        (pin "1") 
        (pintype "passive")) 
      (node 
        (ref "C2") 
        (pin "1") 
        (pintype "passive")) 
      (node 
        (ref "D1") 
        (pin "1") 
        (pinfunction "K") 
        (pintype "passive")) 
      (node 
        (ref "L1") 
        (pin "1") 
        (pinfunction "IN") 
        (pintype "power_in"))) 
    (net 
      (code "11") 
      (name "Net-(J1-Pin_1)") 
      (node 
        (ref "J1") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive")) 
      (node 
        (ref "J2") 
        (pin "1") 
        (pintype "passive")) 
      (node 
        (ref "J3") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive"))) 
    (net 
      (code "12") 
      (name "unconnected-(A1-Pin_16-Pad16)") 
      (node 
        (ref "A1") 
        (pin "16") 
        (pinfunction "Pin_16") 
        (pintype "passive"))) 
    (net 
      (code "13") 
      (name "unconnected-(A1-Pin_17-Pad17)") 
      (node 
        (ref "A1") 
        (pin "17") 
        (pinfunction "Pin_17") 
        (pintype "passive"))) 
    (net 
      (code "14") 
      (name "unconnected-(A1-Pin_18-Pad18)") 
      (node 
        (ref "A1") 
        (pin "18") 
        (pinfunction "Pin_18") 
        (pintype "passive"))) 
    (net 
      (code "15") 
      (name "unconnected-(A1-Pin_19-Pad19)") 
      (node 
        (ref "A1") 
        (pin "19") 
        (pinfunction "Pin_19") 
        (pintype "passive"))) 
    (net 
      (code "16") 
      (name "unconnected-(A1-Pin_20-Pad20)") 
      (node 
        (ref "A1") 
        (pin "20") 
        (pinfunction "Pin_20") 
        (pintype "passive"))) 
    (net 
      (code "17") 
      (name "unconnected-(A1-Pin_21-Pad21)") 
      (node 
        (ref "A1") 
        (pin "21") 
        (pinfunction "Pin_21") 
        (pintype "passive"))) 
    (net 
      (code "18") 
      (name "unconnected-(A1-Pin_22-Pad22)") 
      (node 
        (ref "A1") 
        (pin "22") 
        (pinfunction "Pin_22") 
        (pintype "passive"))) 
    (net 
      (code "19") 
      (name "unconnected-(A1-Pin_25-Pad25)") 
      (node 
        (ref "A1") 
        (pin "25") 
        (pinfunction "Pin_25") 
        (pintype "passive"))) 
    (net 
      (code "20") 
      (name "unconnected-(A1-Pin_26-Pad26)") 
      (node 
        (ref "A1") 
        (pin "26") 
        (pinfunction "Pin_26") 
        (pintype "passive"))) 
    (net 
      (code "21") 
      (name "unconnected-(A1-Pin_28-Pad28)") 
      (node 
        (ref "A1") 
        (pin "28") 
        (pinfunction "Pin_28") 
        (pintype "passive"))) 
    (net 
      (code "22") 
      (name "unconnected-(A1-Pin_30-Pad30)") 
      (node 
        (ref "A1") 
        (pin "30") 
        (pinfunction "Pin_30") 
        (pintype "passive"))) 
    (net 
      (code "23") 
      (name "unconnected-(A2-Pin_1-Pad1)") 
      (node 
        (ref "A2") 
        (pin "1") 
        (pinfunction "Pin_1") 
        (pintype "passive"))) 
    (net 
      (code "24") 
      (name "unconnected-(A2-Pin_2-Pad2)") 
      (node 
        (ref "A2") 
        (pin "2") 
        (pinfunction "Pin_2") 
        (pintype "passive"))) 
    (net 
      (code "25") 
      (name "unconnected-(A2-Pin_3-Pad3)") 
      (node 
        (ref "A2") 
        (pin "3") 
        (pinfunction "Pin_3") 
        (pintype "passive"))) 
    (net 
      (code "26") 
      (name "unconnected-(A2-Pin_7-Pad7)") 
      (node 
        (ref "A2") 
        (pin "7") 
        (pinfunction "Pin_7") 
        (pintype "passive"))) 
    (net 
      (code "27") 
      (name "unconnected-(A2-Pin_8-Pad8)") 
      (node 
        (ref "A2") 
        (pin "8") 
        (pinfunction "Pin_8") 
        (pintype "passive"))) 
    (net 
      (code "28") 
      (name "unconnected-(A2-Pin_9-Pad9)") 
      (node 
        (ref "A2") 
        (pin "9") 
        (pinfunction "Pin_9") 
        (pintype "passive"))) 
    (net 
      (code "29") 
      (name "unconnected-(A2-Pin_10-Pad10)") 
      (node 
        (ref "A2") 
        (pin "10") 
        (pinfunction "Pin_10") 
        (pintype "passive"))) 
    (net 
      (code "30") 
      (name "unconnected-(A2-Pin_11-Pad11)") 
      (node 
        (ref "A2") 
        (pin "11") 
        (pinfunction "Pin_11") 
        (pintype "passive"))) 
    (net 
      (code "31") 
      (name "unconnected-(A2-Pin_12-Pad12)") 
      (node 
        (ref "A2") 
        (pin "12") 
        (pinfunction "Pin_12") 
        (pintype "passive"))) 
    (net 
      (code "32") 
      (name "unconnected-(A2-Pin_14-Pad14)") 
      (node 
        (ref "A2") 
        (pin "14") 
        (pinfunction "Pin_14") 
        (pintype "passive"))) 
    (net 
      (code "33") 
      (name "unconnected-(A2-Pin_15-Pad15)") 
      (node 
        (ref "A2") 
        (pin "15") 
        (pinfunction "Pin_15") 
        (pintype "passive")))))